<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">/* 1281 type user buffer */

DEFINE_STRUCT  USER_BUFFER  12
  ELEM         1  SHORT    version                               none
  ELEM         1  SHORT    max_avgs                              none
  ELEM         1  SHORT    first_bin                             none
  ELEM         1  SHORT    n_bins                                none
  ELEM        20  SHORT    avg_uv                                mm/s
  ELEM         1  SHORT    set                                   deg*E-1
  ELEM         1  SHORT    drift                                 kts*E-2
  ELEM         1  SHORT    position_source                       none
  ELEM         1  SHORT    dr_time                               s
  ELEM         1  STRUCT   fix                                   none
  ELEM         1  LONG     time                                  s
  ELEM         1  STRUCT   gps_status                            none

DEFINE_STRUCT  fix  21
  ELEM         1  SHORT    ref_u                                 mm/s
  ELEM         1  SHORT    ref_v                                 mm/s
  ELEM         1  SHORT    ref_count                             none
  ELEM         1  SHORT    sat_id                                none
  ELEM         1  LONG     pc_time                               s
  ELEM         1  LONG     fix_time                              s
  ELEM         1  LONG     lon                                   sec*E-2
  ELEM         1  LONG     lat                                   sec*E-2
  ELEM         1  LONG     antenna                               m*E-1
  ELEM         1  SHORT    dr_dist                               nm*E-2
  ELEM         1  SHORT    dr_dir                                deg*E-1
  ELEM         1  SHORT    sigma_lon                             m
  ELEM         1  SHORT    sigma_lat                             m
  ELEM         1  BYTE     used                                  none
  ELEM         1  BYTE     q1                                    none
  ELEM         1  BYTE     q2                                    none
  ELEM         1  BYTE     q3                                    none
  ELEM         1  BYTE     elevation                             deg
  ELEM         1  BYTE     iterations                            none
  ELEM         1  BYTE     dop_count                             none
  ELEM         1  BYTE     spare                                 none

DEFINE_STRUCT  gps_status 14
  ELEM         1  SHORT   received                               none
  ELEM         1  BYTE    nsat                                   none
  ELEM         1  BYTE    quality                                none
  ELEM         3  BYTE    track_status[3]                        none
  ELEM         1  BYTE    state                                  none
  ELEM         1  BYTE    mode                                   none
  ELEM         1  BYTE    hdop                                   none
  ELEM         1  SHORT   dopN                                   none
  ELEM         1  SHORT   dopE                                   none
  ELEM         1  SHORT   dopV                                   none
  ELEM         1  SHORT   OscBias                                m/s*E-1
  ELEM         1  SHORT   V                                      Kts*E-2
  ELEM         1  SHORT   U                                      Kts*E-2
  ELEM         1  SHORT   altitude                               m*E-1

</pre></body></html>